{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":3,"n_cols":6,"rows_kept":3,"flags":["formulas_cached_only"]}
[]
["序\n号","设备名称","型号","单位","数量","备注"]
[1,"高频雷达料位计","除尘灰，频率：80G.Hz,平面透镜天线，发射角度：3°。0~10.3m,24VDC,4~20mA输出，两线制，带数显。带HART通讯协议，IP67,带DN150配对法兰及螺栓紧固\n","个",3,"注明品牌"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}